



**NST31042 – Practical for Scaling and Connecting**


Academic year 2019/2020





























Q2.




























Q3.


















4.










5.



Discussion:

* From this session I have learn that how the network has been preconfigured .
* Try to fixe the problems and finally configured and ping them

References:

Lab session

<https://www.cisco.com/c/en/us/td/docs/ios-xml/ios/iproute_ospf/configuration/xe-16/iro-xe-16-book/iro-cfg.html>