



SEU-IS-19-ICT-046


LABREPORT 6








































































Discussion:

From this session I have learnt that how does OSPF configuration works

References:

Practical session

https://www.networkstraining.com/configuring-ospf-on-cisco-routers/